**Specifications**

Machine bed has three guideways;and high rigidity,high load capacity and high accuracy.

        heavy-duty horizontal lathe

|  |  |  |
| --- | --- | --- |
| Main specification | unit | CC61160/180/200/220/250 |
| swing over bed | mm(in) | 1600/1800/2000/2200/2500 |
| swing over carriage | mm(in) | 1250/1400/1600/1800/2000 |
| max.turning length | mm(in) | 5000~20000 |
| max. load between centers | ton | 63 |
| bed width | mm(in) | 1600/2050 |
| spindle speed | rpm | 0.8~160-0.63~125 |
| spindle motor | kW | 75,90,110,125 |