. Specifications Intro:

1. Step Width (mm): 600 /800/ 1000

2. Horizontal Step (pcs): 2/3

II. Steps materials 1.Steps materials divide Stainless steel & Aluminium alloy (both with Yellow Resin Demarcation Line optional )

a).Stainless steel Step: Surface bright, high strength, corrosion resistance, easy to clean and maintenance, weight more than aluminum

b).Aluminium alloy Step: Surface bright, Light weight, High strength, Corrosion resistance, Easy to clean and maintenance

III. Qualification Profile:

1. SEPROS provides escalators, automatic sidewalk products and relevant components since 1996.

2. In July, 2009, our company renewed the manufacturing licence of special equipment (escalators and automatic sidewalks).

3. In October, 2009, Enterprise Resource Planning System of our company was launched officially. Our company stepped into new a period of information management.

4. In April, 2010, we launched our official website. Website: www.sepros.cn.

5. In October, 2010, our products passed CE certification .

6. In November, 2010, our quality management system is upgraded to ISO9001: 2008.

7. All of the installation and technical staff have been professional and technical guidance, with rich experience for the elevator industry

8. Products sell well in Europe, the Middle East, Southeast Asia and other countries, has a wealth of overseas experience in customer service.

9. In the future, we will do our best to provide customers with more superior products, relevant components and more excellent after-sales service relying on more than ten years' professional experience in dealing with escalators and automatic sidewalks.